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	Pos no.
	Quantity
	Unit
	Unit price
	
	Total amount
	



	1.0 
	
Building automation system for incorporation into building management systems 

An automation controller with the following profile should be used for connecting emergency exit control units, electric locks, automatic door systems, smoke and heat extraction systems and automatic window systems as well as devices from adjoining product groups which are designed for using typical building automation functions:

· A BACnet-Building Controller (B-BC) BACnet device must be provided
· Proof of the product's tested conformity to the BACnet standard ISO 16484-5 must be provided


	1.1 

	
myGEZE Control System

The basic controller is a high-performance control unit with a switched Ethernet port that supports the BACnet protocol. 
Type B-BC (BACnet Building Controller) BACnet controller
BACnet Protocol Revision 14

for integrating GEZE fieldbus devices

comprising:

…….  pc.	myGEZE Control basic controller, embedded PC / control unit
                         incl. GEZE Library software licence 

........  pc.	OPC UA as an additional interface (licence) 

........  pc.	GEZE automatic door drive units (DCU)  
                          e.g. GEZE Powerturn, Slimdrive SL NT, Revo.PRIME, etc.

........  pc.	GEZE RWS emergency exit door control unit TZ32x
                         
........  pc.	GEZE automatic swing door drive with emergency exit door control unit
                          (DCU+TZ32x) as part of a system

........  pc.	GEZE SHEV MBZ 300 SHEV control panel
		                          
........  pc.	Digital input for connecting binary input signals
                         based on potential-free contacts 

........  pc.	Digital output for connecting digital output signals
                         based on potential-free contacts, 24V DC

........  pc.	GEZE fire door holder on the controller 

........  pc.	GEZE IO 420 CAN bus module, with 4 each digital inputs and outputs 

........  pc.	GEZE IQ box KNX for GEZE IQ Window Drives 

Including a suitable top hat rail housing with a power supply unit, as well as the necessary auxiliary terminals for internal potential distribution, bus power supply and termination.


The type and number of terminal systems used depend on the product systems connected to them.

Supply voltage: 230V AC 

incl. the following services:

· Project planning and interface configuration of the offered networking system according to GEZE standard.

· Mechanical assembly, electrical connection, commissioning

· Electrical circuit diagram for the controller 

· Project monitoring and coordination 

.........................  Piece                   ..............................  €             ..............................  €



	1.2 
	
myGEZE OPC UA (licence) 
 
Licence option myGEZE Control as an OPC UA server for communication using the OPC UA standard protocol. 

........................  Piece                   ..............................  €             ..............................  €



	1.3 
	
myGEZE Viewer (licence) 
 
GEZE control panel software myGEZE Viewer – a software application for the browser-based display and operation of connected GEZE product systems in the fields of rescue route technology and automatic door operators

Devices to be illustrated: …….. (Number 1–50)

........................  Piece                   ..............................  €             ..............................  €



	1.4 

	
Optional additional services:

Creation of project-specific wiring schematics for product systems

The service includes: 
· Creation of one basic diagram per door type
· Creation of a wiring schematic for the installed door, window and safety technology product systems
· A change index is included; additional changes charged separately

            ........................  Option                   ..............................  €             .............................  €
Additional/added planning and coordination meetings / design meetings with the client and other subsections during the planning phase

........  Piece 	as online appointment

........  Piece 	as appointment on site, incl. journey

........................  Option                   ..............................  €             ............................  €


Hourly labour and additional trip to site
Hourly charges for additional work and services. Billing based on time and work performed, with documentation.
...................1 Hour  Option                   .......................  €             ..........................  €

...................1 Approach  Option                   .......................  €             ........................... €




	1.5 
	[bookmark: _Hlk135207916]
Accessories

CAN interface  
 
CAN extension module galvanically isolated for automatic sliding door, revolving door and swing door drives as an interface for connection to the GEZE building management system myGEZE Control.
Assembly, electrical connection and CAN addressing

............................  Option                   ..............................  €             ..............................  €
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