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	Pos no.
	Quantity
	Unit
	Unit price
	
	Total amount
	



	1.0 
	             .........................  pc.                   ..............................  €             ..............................  €
GEZE Revo.PURE: revolving door system in three- or four-leaf design
with freely selectable diameter up to 3800 mm, TÜV type-approval in accordance with EN 16005, with a canopy height of 200 mm, drive fully integrated into the ceiling construction. Side walls and door leaves with fine frame in a light, inviting look.
Drive types:
(  ) manual operation of the door
or
(  ) fully automatic GEZE revolving door system (activation via movement detector)
Microprocessor-controlled, electromechanical drive with variably adjustable speed, power supply: 230 V / 50 Hz / 60 Hz / 330 W / 10 A
Keypad programme switch for adjusting the modes of operation
Connection to a building automation control system with preset inputs and outputs possible
tested in accordance with EN 16005:2013-01
Construction dimensions:
(  ) Outside diameter:  ..................mm (freely selectable between 1880 and 3880 mm)
(  ) Clear passage height: ....  ..    mm (up to 3000 mm, higher on request)
(  ) Total height of door system: ...mm
(  ) Floor recess: ................   ....... mm (min. 60 mm)
Note: Mounting distance: 40 mm on all sides
Door position in façade:
(  ) central
(  ) off-centre, offset in relation to the façade ….. mm
Model type:
(  ) three-leaf
(  ) four leaf
Leaves:
Fixed door leaves, fine-framed, 80 mm visible width to mount laminated safety glass
Side walls fine-framed made of GEZE aluminium profiles with 80 mm visible width. Side wall joint with integrated cavity for cable routing upwards and/or downwards. Side wall filling with:
(  ) curved LSG 8/10 mm, clear
Aluminium ceiling construction:
(  ) 200 mm standard height
or
(  ) ___ mm with elevated ceiling construction (200 – 600 mm) with circumferential canopy cover made of curved aluminium sheets 
Roof covering outside:
(  ) Visible sheet covering made of 1.5 mm aluminium in the same colour as the system
or
(  ) Waterproof with 2 waterspouts (flat roof without gradient)
Roof covering inside:
Visible sheet covering made of 1.5 mm aluminium in the same colour as the system
Soffit:
(  ) Consisting of aluminium circular segments in the same colour as the system incl. inspection opening
Surface of the light metal parts:
(  ) Powder coating according to RAL
or
(  ) LM anodised E6/EV1
or
(  ) Colour anodised ............
or
(  ) Coated with ground stainless steel, grain 240 (1.4301)
or
(  ) Coated with polished stainless steel (1.4301)
Floor ring:
(  ) GEZE 360° stainless steel (V2A) floor ring made of rectangular tube 30 x 30 x 2 mm. The floor ring also serves as edging of the flooring with
(  ) Sheet metal base from 100 mm
and/or
(  ) Loose/fixed flange according to DIN 18533
or
(  ) Direct installation of the self-supporting side wall construction to the top edge of the finished floor. Note: Only possible with a sufficiently load-bearing and even finished floor level. (+/- 1 mm).
Note: Building sealing is a third-party service.
Floor covering:
(  ) GEZE entrance mat, anthracite, 22 mm, more colours available on request!
or
(  ) Without floor covering
Delivery and installation:
Wiring to be carried out on site according to GEZE cable plan by an electrical contractor.
Installation, commissioning and operator training as well as handover of documentation in accordance with EN 16005 by factory technicians or service partners.


	1.1 
	             .........................  pc.                   ..............................  €             ..............................  €
Night-time closer with continuous 4-point guide (optional position)
(  ) GEZE night-time closer sliding doors externally guided, manual, lock possible from inside and outside.
(  ) fine-framed in LSG 8/10 mm, clear
Locking of the night-time closer sliding doors using:
(  ) Hook bolt lock (no lock monitoring possible, 3-point guide)


	1.2 
	             .........................  pc.                   ..............................  €             ..............................  €
Locking (optional position)
(  ) Without locking mechanism
or
(  ) Manual bolt lock installed on top of the door leaf
or
(  ) Electro-mechanical locking mechanism (two-stage), the door remains in its previous state in case of a power failure (only for automatic doors) 
Note:
When using a night-time closer, the turnstile does not need to be locked.


	1.3 
	             .........................  pc.                   ..............................  €             ..............................  €
Handles (optional position)
(  ) ground, horizontal stainless steel back to back straight D handles, installation on the profile, length: …..
or
(  ) ground, vertical stainless steel back to back straight D handles, installation on the profile, length: …..


	1.4 
	             .........................  pc.                   ..............................  €             ..............................  €
Operation (optional position)
GEZE key switch to lock the programme switch in order to prevent unauthorised changing of the mode of operation, IP40 rating
(  ) Surface-mounted   (  ) Flush-mounted


	1.5 
	             .........................  pc.                   ..............................  €             ..............................  €
Push pad (optional position)
(  ) Delivery and installation of two GEZE push-padswith wheelchair symbol on the right mullion of the revolving door. When these buttons are pushed, the revolving speed is reduced in order to offer better ease of access and more safety to persons with physical restrictions.
Note:
Can only be used with fully automatic drive.


	1.6 
	             .........................  pc.                   ..............................  €             ..............................  €
Lighting (optional position)
(  ) .....piece LED spotlight (max. 2.6 W per light) integrated in the soffit. Can be activated via
           the building automation control system if needed. 
Or
(  ) ..... piece(s) recess for lighting to be installed on site (diameter = ..... mm)


	1.7 
	             .........................  pc.                   ..............................  €             ..............................  €
Air curtain system (optional position)
(  ) Air curtain system fully integrated into the ceiling construction of the revolving door, incl. discharge channel in the canopy area. Operated using a control panel. Connection to the building automation control system is possible. The minimum canopy height depends on the diameter.
Air curtain system design with:
(  ) Electrical connection:          Heating output: ............KW/ Air volume: .............m³/h
(  ) Hot water connection          Heating output: ............KW/ Air volume: .............m³/h
Note:
We recommend consulting with a specialist planner to dimension and specify the air curtain. It will be connected to the heating system on site.


	1.8 
	             .........................  pc.                   ..............................  €             ..............................  €
Façade connection
(  ) Lateral U profile with connection panels on all sides, 34 mm in the same colour as the system from GEZE incl. installation and sealing.
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