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	1.0 
	             .........................  pcs.                  ..............................  €             ..............................  €

GEZE Revo.PRIME GG all-glass revolving door system in three or four-leaf design
With an outstanding, transparent appearance, freely selectable diameter up to 3000 mm, TÜV type-tested in accordance with EN 16005, with different drive types and multiple available equipment options
Drive types:
(  ) Manual operation of the door
or
(  ) Manually operated door (turnstile) with GEZE speed limiter, i.e. the maximum speed of the revolving door is limited by a safety mechanism in the door.
or
(  ) Manually operated door (turnstile) with GEZE positioning device. After the turnstile has been passed through, the motor gear unit moves it back to its starting position/ end position at very low speed
or
(  ) Fully automatic GEZE revolving door system (activated via movement detectors)
Microprocessor-controlled electromechanical drive with variable speed adjustment, power supply: 230 V / 50 Hz / 330 W / 10 A
Keypad programme switch for adjusting the modes of operation
Connection to a building automation control system with preset inputs and outputs possible
Tested in accordance with EN 16005:2013-01
Opening in floor of building shell: 970 x 900 x 200 mm
Construction dimensions:
(  ) Outside diameter:  ..................mm (freely selectable between 1880 and 3240 mm)
(  ) Clear passage height DH: ....  .. mm (up to 3000 mm, higher on request)
(  ) Total height of door system: ...............mm
(  ) Canopy height: 17.52 mm (height of glass roof)
(  ) Floor recess: ................   ..........mm (min. 200 mm)
Note: Mounting distance: 40 mm all around
Door position in façade:
(  ) central
(  ) off-centre, offset in relation to the façade ….. mm
Design type:
(  ) three-leaf
(  ) four leaf
Leaves:
Rigid door leaves, fine-framed on 3 sides, 65 mm visible width for mounting toughened safety glass
Drum walls:
Fine-framed on 3 sides made of GEZE aluminium profiles with 60 mm visible width. Side screen joint with integrated hollow chamber for cable routing upwards and/or downwards. Side screen filling with curved laminated safety glass 16 mm, clear
Ceiling construction:
(  ) Glass ceiling made of flat 17.52 mm LSG (2 x heat strengthened soda lime silicate glass) clear glass. Outer edges with edge protection. The two glass half-shells are held in place at individual points and have a recess to mount the rotary axis bearing.
Surface of the light metal parts:
(  ) Powder coating according to RAL
or
(  ) LM anodised E6/EV1
or

(  ) Anodized Euras C31, C32, C33, C34, C35

or
(  ) coated with ground stainless steel, grain 240 (1.4301)
or
(  ) coated with polished stainless steel (1.4301)
Floor ring:
(  ) GEZE 360° stainless steel (V2A) floor ring made of rectangular tube 30 x 30 x 2 mm. The floor ring is used as the floor covering edging at the same time. Drive box dimensions: 871 × 614 × 180 mm
(  ) Sheet metal base from 200 mm
and/or
(  ) Loose bolted flange according to DIN 18533
Note: Building waterproofing is a service provided by a third party.
Floor covering:
(  ) GEZE entrance mat, anthracite colour, 22 mm, more colours available on request!
or
(  ) without floor covering
Delivery and assembly:
Wiring to be carried out on site according to GEZE cable plan by an electrical contractor.
Assembly, commissioning and instruction of the operator, as well as handover of documentation in accordance with EN 16005 by factory fitters or service partners.


	1.1 
	             .........................  pcs.                  ..............................  €             ..............................  €

Night-time closer with continuous 4-point guide (optional position)
(  ) GEZE night-time closer sliding doors outside-running, manual, as underfloor roller guide, box size of the underfloor roller guide in the floor approx. 85 x 99 mm (for 3-leaf 120°; for 4-leaf 180°) with connection for on-site floor guide drainage, night sliding doors made of curved 12 mm laminated safety glass, clear, floor bolt lock on sliding leaf (Euro profile cylinder on site), lock from inside and outside.

	1.2 
	             .........................  pcs.                  ..............................  €             ..............................  €

Locking (optional position)
(  ) without locking mechanism
or
(  ) manual locking mechanism with GEZE  espagnolette bolt  lock integrated into the door leaf, including Euro profile half cylinder 
Note: When using a night-time closer, the turnstile locking mechanism is not required.


	1.3 
	             .........................  pcs.                  ..............................  €             ..............................  €

Handles (optional position)
(  ) ground, horizontal stainless steel pull handles, Ø 30 mm, installation directly on the glass, length: …..
or
 (  ) fround, vertical stainless steel pull handles, diameter 30 mm, installation directly on the glass, standard length up to 1500 mm
(  ) ground, vertical stainless steel pull handles, diameter 40 mm, installation directly on the glass, length according to the leaf height


	1.4 
	             .........................  pcs.                  ..............................  €             ..............................  €

Operation (optional position)
GEZE key switch to “lock” the programme switch to prevent unauthorised changing of the mode of operation, IP40 rating
(  ) Surface-mounted   (  ) Flush-mounted


	1.5 
	             .........................  pcs.                  ..............................  €             ..............................  €

Push pad (optional item)
(  ) Delivery and installation of two GEZE push buttons with wheelchair symbol on the right mullion of the revolving door. When these buttons are pushed, the revolving speed is reduced in order to offer better ease of access and more safety to persons with physical restrictions.
Note: Can only be used with fully automatic drive.

	
	

	1.6 
	             .........................  pcs.                  ..............................  €             ..............................  €

Façade connection
(  ) Side U profiles with circumferential connection panels 34 mm in GEZE system colour, including assembly and sealing


	1.7 
	             .........................  pcs.                  ..............................  €             ..............................  €

CAN interface for the connection to the building management

Technical data:
CAN interface galvanically isolated.
CAN extension module for automatic GEZE sliding door, revolving door and swing door drives as interface to connect to the GEZE building management system myGEZE Control.


	1.8 
	             .........................  pcs.                  ..............................  €             ..............................  €

Building automation connection

Building automation and control system 
For the integration of escape door control units, swing door drives, sliding doors and automatic window systems into a building management system for the use of typical building automation and control functions.
An automation controller with the following profile must be used:
BACnet device of the type BACnet Building Controller (B-BC) with tested conformity to the BACnet standard ISO 16484-5
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