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	Unit
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	1.0 
	             .........................  pcs.                   ..............................  €             ..............................  €

GEZE Slimdrive SL for angled façades
Modular, compact automatic linear sliding door, with a drive height of only 70 mm, fine-framed in a sophisticated design for unusual applications, TÜV type-tested in accordance with EN 16005, suitable for an angle of up to 10° from vertical. Larger angles available on request.

Integrated battery for emergency opening and closing in the event of a power failure

Latest software for optional Bluetooth connection to a PC for convenient parameter setting, start-up and maintenance

Intelligent digital control (Category 2 in accordance with DIN EN 954-1 and Performance Level “d” in accordance with DIN EN ISO 13849-1):

- Self-learning

- Optimum convenience thanks to automatic adaptation of door behaviour to through-traffic

- Can be linked and integrated in building systems via CAN-bus

- Independent fault detection and protocol

- Setting possibilities for all door movement parameters

- All functions integrated in one unit, no further modules necessary

- Continuous floor guide with stainless steel carrier rollers, upper edge of floor guide=flush with finished flooring

 mounted on the unfinished floor and embedded in scree.

- Electromagnetic locking, integrated in the drive unit, with manual emergency unlocking

Extremely smooth-running direct current drive for leaf weights up to 100 kg per leaf
Sturdy power supply with integrated all-pole main switch and fuse protection

Static and dynamic power limitation in accordance with EN 16005, as well as static under 150 N in accordance with ASR A1.7 (formerly BGR 232)
Automatic reversal when obstacles are detected

Drive functions (H x D): 70 x 189 mm

Type of installation:

(  ) Wall mounting (the drive must be mounted in a horizontal position!)

or

(  ) Mounting on profile systems/facade (the drive must be mounted in a horizontal position!)

Construction dimensions (dimensions in unfinished state):

Clear overall width LW: ......... mm,

Clear overall height LH: ......... mm,

Passage clearance DB: ......... mm, (1-leaf 700 - 1000 mm)

(2-leaf 900 - 2000 mm)

Passage height DH: ......... ...........mm

Tilt angle from the vertical:...................degrees (larger angles on request!)

Area of application:

No. of leaves

 (  ) single-leaf closing on the left
 (  ) single-leaf closing on the right

 (  ) double-leaf

Fitting:

(  ) moving leaf with ISO or mono-glass fine-framed (up to 100 kg leaf weight):

     (  ) with ISO glass 22 mm made of (  ) ESG or (  ) VSG (depending on angle)

     (  ) with ESG 10 mm

     (  ) with VSG 10 mm

Surface of the light alloy parts of the drive and the moving leaves:

(  ) Powder coating RAL/DB/NCS colours

or

(  ) LM anodised E6/EV1

or

(  ) Colour anodised ............

or

(  ) stainless steel-like anodising (appearance as though ground)

or

(  ) Coated with ground stainless steel, grain 240

or

(  ) Coated with polished stainless steel

Wiring to be carried out on site according to the GEZE cable diagram by an electrical contractor.

Installation, start-up and instruction of the operator as well as documentation handover in accordance with EN 16005 through plant fitters or service partner.

In accordance with EN 16005:

- safety analysis must be carried out as a basis for planning and execution

- an inspection must be carried out at least 1 x year and maintenance at least 1 x year

 

	1.1 
	             .........................  pcs.                   ..............................  €             ..............................  €

Operation

GEZE display programme switch in the AS 500 range for setting the mode of operation as well as for putting the drive into operation and setting parameters, with function keys, 2x 7-segment display, alphanumerical fault display, IP rating IP 40

Operating modes: permanently open, automatic, shop closing, night-locking, off

( ) Surface-mounted ( ) Flush-mounted

or

GEZE key programme switch for setting the operating mode, with function keys, LED matrix display, coded fault display, enclosure rating IP 40, suitable for switch programmes with 55 x 55 mm switch insert

Modes of operation: off, permanently open, automatic, shop closing, night-locking

(  ) Surface-mounted   (  ) Flush-mounted
or

GEZE mechanical programme switch for setting the operating mode, with rotary knob, LED fault display, enclosure rating IP 40, suitable for switch programmes with 55 x 55 mm switch insert

Modes of operation: off, permanently open, automatic, shop closing, night-locking

(  ) Surface-mounted   (  ) Flush-mounted
or

GEZE mechanical programme switch for setting the operating mode, with key, LED fault display, enclosure rating IP 40, suitable for switch programmes with 55 x 55 mm switch insert

Modes of operation: off, permanently open, automatic, shop closing, night-locking

(  ) Surface-mounted   (  ) Flush-mounted



	1.2 
	             .........................  pcs.                   ..............................  €             ..............................  €

Operation (optional position)

GEZE key switch to “lock” the programme switch to prevent unauthorised changing of the operating mode, enclosure rating IP 40

(  ) Surface-mounted   (  ) Flush-mounted



	1.3 
	             .........................  pcs.                  ..............................  €             ..............................  €
Activation and protection (optional position)
GC 363+ combined detector with direction detecting radar movement detector for activation and active infrared detector with two light curtains for protection of the opening or closing area in accordance with EN 16005, IP54 rating, 10 possible light curtain configurations
Version:
( ) black
( ) according to RAL
(  ) outside   (  ) inside
Accessories:
(  ) outside: weather hood to protect the sensor from the interference of rain
(  ) Ceiling installation bracket
(  ) Ceiling installation kit for integrating the sensor in the ceiling

(  ) Smart Daisy Chain Hub for series connection of up to three sliding door sensors


	1.4 
	             .........................  pcs.                  ..............................  €             ..............................  €
Activation and protection (optional position)
GC 365 combined detector with direction detecting radar movement detector for activation and active infrared detector with two light curtains for protection of the opening or closing area in accordance with EN 16005, IP54 rating, 4 possible light curtain configurations
Version:
( ) black
( ) outside   ( ) inside
Accessories:
( ) outside: weather hood to protect the sensor from the interference of rain
( ) Ceiling installation bracket
( ) Ceiling installation kit for integrating the sensor in the ceiling
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	             .........................  pcs.                   ..............................  €             ..............................  €

Activation (optional position)

GEZE elbow switch, plastic, IP rating IP 30
Dimensions: 90 x 180 x 23 mm 
( ) white  ( ) stainless steel
( ) optional transmitting module 
( ) Surface-mounted  ( ) Rear panel for attaching the elbow switch to glass (in connection with the transmitting module)
or
GEZE elbow switch, LS990, IP rating IP 30
Dimensions: 81 x 223 x 51 mm
( ) white  ( ) stainless steel
( ) optional transmitting module 
( ) Surface-mounted ( ) Flush-mounted
or
GEZE elbow switch, stainless steel, IP rating IP 65
Dimensions: 72 x 250 x 17 mm 
( ) Surface-mounted
 
or
GEZE non-contact proximity switch (radar)
Plastic with antimicrobial surface, IP rating IP65, multi-colour LED feedback, adjustable acoustic feedback. Additional input to actively change the LED colour.

Dimensions: 80 x 80  mm

( ) Flush mounting 12 mm deep
( ) Surface mounting 21 mm deep
( ) Variant for WC
 
or
GEZE LED sensor push button, plastic, IP rating IP 69K
round, diameter: 100 mm
( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm
 
or
GEZE LED sensor push button, glass, IP rating IP 69K
round, diameter: 100 mm
( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm
or
GEZE LED sensor foot switch, glass, IP rating IP69K

Dimensions: 100 x 100 x 3 mm

( ) flush-mounting

( ) vertically adjustable installation base for depths of up to 215 mm from the unfinished floor
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	             .........................  pcs.                   ..............................  €             ..............................  €

Activation (optional position)

GEZE wireless programme with secure rolling code encryption for wireless drive activation (range of approx. 30 m in the building).

Transmitter:

(  )   Wireless transmitter with 1 key, enclosure rating IP 54 and wall fixing

(  )   Wireless transmitter with 2 keys, enclosure rating IP 54 and wall fixing

(  )   Wireless transmitter with 4 keys, enclosure rating IP 54 and wall fixing

(  )   Wireless transmitter module for optional integration in the GEZE elbow switch
Radio receiver:

(  )   Radio receiver module with 2 outputs, 24 V, pulse mode or pulse and

       permanent mode for mounting in the drive or in a flush-mounted socket with enclosure rating IP 20
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	             .........................  pcs.                   ..............................  €             ..............................  €

Activation (optional position)

GEZE GCER 300, 1-door SET
Access control solution with RFID reader and PIN keypad in stand-alone operation for controlling one door (can be extended to 2 doors). RFID frequency 13.56 MHz. Authorisation is granted through master ID cards in combination with PIN keyboard directly at the reader. Up to 200 persons/ID cards can be authorised. If individual ID cards are lost or become faulty, they can simply be deleted from the system (selective deletion). Two authorisation types for short-time release or continuous release (office function). Configurable door release time. Variable PIN length. Communication between reader and control unit takes place by encrypted data transfer. Functions such as interlocking door system or dementia adjustable. Release buttons can be connected.
Set comprising:
1 pc. GEZE GCER 300 I/O Box (ID no. 185707)
1 pc. GEZE GCVR 300 T, RFID reader flush-mounted (ID no. 185708)
2 pc. GEZE GCER 300 system card master (ID no. 185713)
10 pc. GEZE RFID ID card (ID no. 185711)
Optional
GEZE GCVR Touch 300 T, RFID reader flush-mounted (ID no. 187108)
GEZE RFID key fob (ID no. 185712)
GEZE GCER AP surface-mounted frame (Id. no. 130024)

or

GEZE GCER 300 Light, 1-door SET

Access control solution with RFID reader and PIN keyboard in stand-alone operation with a relay output for controlling one door located in the secured inner area. RFID frequency 13.56 MHz. Authorisation is granted through master ID cards in combination with PIN keyboard directly at the reader. Up to 200 persons/ID cards can be authorised for short-time release. If individual ID cards are lost or become faulty, they can simply be deleted from the system (selective deletion). Configurable door release time. Variable PIN length. Communication takes place via encrypted data transfer.
Set comprising:
1 pc. GEZE GCER 300 Light, RFID reader flush-mounted (ID no. 185710)
1 pc. GEZE GCER 300 system card master (ID no. 185713)
10 pc. GEZE RFID ID card (ID no. 185711)
Optional
GEZE RFID key fob (ID no. 185712)
GEZE GCER AP surface-mounted frame (ID no. 130024)

Accessories for GCER 300 / GCER 300 Light
Plug-in power supply NT 1.0 A – 24 V DC (optional)
Primary:  230 V AC, 50 Hz
Secondary: 24 V DC (+/- 5 %) / 1 A
(ID no. 130025)

Power supply NT 1.1 A – 24 V DC flush-mounted (optional)
For installation in deep standard flush-mounted boxes
Primary:  230 V AC, 50 Hz
Secondary: 24 V DC / 1.1 A
(ID no. 151426)
Power supply NT 1.5 A – 24 V DC HA (optional)
For installation on top hat rails 
Primary: 230 V AC, 50 Hz
Secondary: 21.6 – 26.4 V DC / 1.5 A
(ID no. 151425)
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Activation (optional position)

GEZE key switch outside (enclosure rating IP 54) with or without profile half cylinder and switch function 
(  ) Surface-mounted   (  ) Flush-mounted
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	             .........................  pcs.                   ..............................  €             ..............................  €

Activation (optional position)

GEZE key switch outside (enclosure rating IP 54) with or without profile half cylinder and catch function for the fire brigade 
(  ) Flush-mounted



	1.10 
	             .........................  pcs.                   ..............................  €             ..............................  €

Activation (optional position)

GEZE key switch outside (enclosure rating IP 54), prepared for on-site profile half cylinder from the locking system as well as 1 push button with key symbol for opening from the inside. On contact, the system opens from its locked position once outwards and inwards, and locks again after the leaf has reached the closed position.



	1.11 
	             .........................  pcs.                   ..............................  €             ..............................  €

Activation (optional position)

GEZE auxiliary button for limited opening width
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	             .........................  pcs.                   ..............................  €             ..............................  €

Protection

GEZE safety leaf for protecting against shearing and nipping spots in accordance with EN 16005 with post-rail structures (depending on the distance between post surface and facade glassing) behind the moving leaf, leaf made of 10 mm ESG incl. fitting

alternatively:

(  ) sensor-controlled fixed panel protection using 3D light curtain (depending on angle)
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	             .........................  pcs.                   ..............................  €             ..............................  €

Protection (optional position)

GEZE self-monitoring system double 3D light curtain to secure the closing or opening area in accordance with EN 16005, enclosure rating IP 54 (for people in need of special protection, depending on angle)

(  ) outside   (  ) inside
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	             .........................  pcs.                   ..............................  €             ..............................  €

Protection (optional position)

GEZE emergency stop switch with glass pane and light, for switching off the mains voltage, enclosure rating IP 20

An emergency command device (emergency stop switch) is not essential in accordance with EN 16005.

(  ) Surface-mounted   (  ) Flush-mounted
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	             .........................  pcs.                   ..............................  €             ..............................  €

Protection (optional position)

GEZE emergency stop switch with illuminated mushroom button for emergency opening or unlocking, enclosure rating IP 40

An emergency command device (emergency stop switch) is not essential in accordance with EN 16005.

(  ) Surface-mounted   (  ) Flush-mounted
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CAN interface for the connection to the building management

Technical data:
CAN interface galvanically isolated.
CAN extension module for automatic GEZE sliding door, revolving door and swing door drives as interface to connect to the GEZE building management system myGEZE Control.
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Building automation connection

Building automation and control system 
For the integration of escape door control units, swing door drives, sliding doors and automatic window systems into a building management system for the use of typical building automation and control functions.
An automation controller with the following profile must be used:
BACnet device of the type BACnet Building Controller (B-BC) with tested conformity to the BACnet standard ISO 16484-5

myGEZE Control System
...... Piece basic controller as a powerful embedded PC that supports the BACnet protocol. BACnet controller of type B-BC (BACnet Building Controller / protocol audit 14)
for the integration of GEZE field bus devices. The number of fieldbus devices is specified in the specifications.

The system must be able to provide the following components (incl. software licence):

· myGEZE Control basic controller, embedded PC incl. GEZE Library 
· Terminal system for connecting the GEZE CAN bus 
· Terminal system for the connection of GEZE window technology based on 
             the IQ box KNX  
· Terminal system for connecting digital binary input signals to
             Basis of potential-free contacts 
· Terminal system for connecting digital output signals based on
potential-free door closer or changeover contacts 24 V DC     
The number of terminal systems is to be determined by the supplier on the basis of the tendered products at field level.
In top hat rail housing, incl. power supply unit, required auxiliary terminals for internal potential distribution, bus supply and bus termination.
Standard housing dimensions:  W x H x D 300 x 400 x 200 mm 
Supply voltage: 230 V AC 
incl. the following services:
· Project planning and interface configuration of the offered networking system according to GEZE standard.

· Mechanical assembly, electrical connection, commissioning
              ...........  Option                   ..............................  €             ..............................  €
Optional additional services:

Creation of project-specific wiring schematics for product systems

The service includes: 
· Creation of one basic diagram per door type
· Creation of a wiring schematic for the installed door, window and safety technology product systems
· A change index is included; additional changes charged separately
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