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	1.0 
	             .........................  pcs.                  ..............................  €             ..............................  €

GEZE Slimdrive SCR-FR
Modular, compact automatic curved sliding door (360°) with a drive height of only 70 mm for use in emergency exit routes, TÜV type-tested in accordance with EN 16005, in 2-motor technology, fine-framed in light-coloured transparent design, unusually spacious, with a freely selectable diameter between 2200 mm and 3500 mm.

Redundant emergency exit function through 2-motor technology, with duplicate processing system and low-maintenance

Monitored rechargeable battery for emergency opening in the event of a power failure

Latest software for optional Bluetooth connection to a PC for convenient parameter setting, commissioning and after-sales service maintenance

Redundant digital control performance level D according to DIN EN ISO 13849-1):

- Self-learning

- Optimum convenience thanks to automatic adaptation of door behaviour to traffic

- Can be networked and integrated in building systems via CAN-bus

- Independent fault detection and protocol

- Adjustment options for all door movement parameters

- All functions integrated in one unit, no further modules necessary

- Stainless steel floor guide embedded in the floor

Two extremely quiet running direct current drives, for leaf weights up to 120 kg

Robust power supply with integrated all-pole main switch and fuse protection

Static and dynamic power limitation according to EN 16005, as well as static under 150 N in accordance with ASR A1.7
Automatic reversal when obstacles are detected

Additional variants for more safety and convenience:

(  ) FR-RWS

For use in emergency exit systems with locked escape route and emergency opening switch, with TÜV report for enabling in individual cases (has to be applied for by the client) *

(  ) FR-LL

For locked one-way or shop closed function, TÜV type-tested

(  ) FR-DUO

With emergency exit function in both directions, TÜV type-tested

*The use of an emergency push button is compulsory for the RWS operating mode, with all other variants an emergency command device (emergency stop switch) does not have to be used.

Activation and protection (optional position)
GC 363+ combined detector with direction detecting radar movement detector for activation and active infrared detector with two light curtains for protection of the opening or closing area in accordance with EN 16005, IP54 rating, 10 possible light curtain configurations

GC 339+ active infrared detector with two light curtains for protecting the opening or closing area in accordance with EN 16005, IP54 rating, 10 possible light curtain configurations
Version:
( ) black
( ) according to RAL
Construction dimensions (dimensions in unfinished state):

Outside diameter:                   .............mm, freely selectable between 2000 and 3500 mm
Clear passage height PH:       .............mm

Total height of door system:             ....mm

Passage clearance PC:                 .......mm

Note: Other dimensions on request!

Fine-framed drum walls made of GEZE profile systems for mounting:
(  ) Curved laminated safety glass 10 mm, clear

or

(  ) Curved thermally insulated panel lining, 22 mm thick

or

(  ) curved ISO laminated safety glass 22 mm, clear, Ug value 3.0, height up to 2500 mm
Fine-framed moving leaf of GEZE profile systems for the accomodation of:

(  ) curved laminated safety glass 10 mm, clear
or
(  ) curved ISO laminated safety glass 22 mm, clear, Ug value 3.0, height up to 2500 mm
Aluminium ceiling construction:
(  ) Standard height 70 mm

or

(  ) Raised ceiling canopy .............mm, with perimeter canopy cover made of curved aluminium sheets

Roof covering outside:

(  ) Metal cover plate

or

(  ) Waterproof roof with 2 water spouts (flat roof without gradient)

or

(  ) Glass roof with metal cover over the drive unit

Roof covering inside:

(  ) Metal cover plate

or

(  ) Glass roof with metal cover over the drive unit

Surface of the light alloy parts:

(  ) Powder coating RAL colours

or

(  ) LM anodised E6/EV1

or

(  ) Colour anodised Euras C31, C32, C33, C34, C35
or

(  ) Coated with ground stainless steel, grain 240

or

(  ) Coated with polished stainless steel

Floor ring:
(  ) GEZE 360° stainless steel (V2A) floor ring made of rectangular tube 30 x 30 x 2 mm. The floor ring serves both as a floor covering border and floor guide.

        (  ) sheet metal base from 100 mm
or
  ) Loose/fixed flange in accordance with DIN 18533
and/or

(  ) Floor plate with discharge nozzle

Note: The insulation of the building is a contracted service and must be carried out on site.

Floor cover:
(  ) GEZE floor mat, anthracite colour, 22 mm, more colours available on request!

or
(  ) EMCO floor mat, anthracite colour, 22 mm, more colours available on request!
or

(  ) Floor cover to be carried out on site

Wiring to be carried out on site according to the GEZE cable plan by an electrical contractor.

Installation, commissioning and instruction of the operator as well as documentation handover in compliance with EN 16005 through plant fitters or service partner.

In compliance with EN 16005:

- Safety analysis must be carried out as a basis for planning and execution

- An inspection must be carried out at least 1 x year and after-sales service maintenance at least 2 x year
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	             .........................  pcs.                  ..............................  €             ..............................  €

Operation

GEZE display programme switch in the AS 500 range for setting the mode of operation as well as for commissioning and parameterisation of the drive, with function keys, 2x 7-segment display, alphanumerical fault display, IP rating IP 40
Operating modes: permanently open, automatic, shop closing, night-locking, off

( ) Surface-mounted ( ) Flush-mounted

or

GEZE key programme switch for setting the operating mode, with control keys, LED dot display, coded error display, IP rating IP 40, suitable for switch product ranges with 55 x 55 mm switch insert

Operating modes: off, permanently open, automatic, shop closing-time, night-locking
(  ) Surface-mounted   (  ) Flush-mounted
According to AutSchR and DIN 16005 the programme switch must be secured against unauthorised adjustment on FR doors:

GEZE key switch to “lock” the programme switch to prevent unauthorised changing of the operating mode, IP rating IP 40

(  ) Surface-mounted   (  ) Flush-mounted
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Activation (optional position)

GEZE elbow switch, plastic, IP rating IP 30

Dimensions: 90 x 180 x 23 mm 

( ) white  ( ) stainless steel

( ) optional transmitting module 

( ) Surface-mounted  ( ) Rear panel for attaching the elbow switch to glass (in connection with the transmitting module)

or

GEZE elbow switch, LS990, IP rating IP 30

Dimensions: 81 x 223 x 51 mm

( ) white  ( ) stainless steel

( ) optional transmitting module 

( ) Surface-mounted ( ) Flush-mounted

or

GEZE elbow switch, stainless steel, IP rating IP 65

Dimensions: 72 x 250 x 17 mm 

( ) Surface-mounted

 
or
GEZE non-contact proximity switch (radar)
Plastic with antimicrobial surface, IP rating IP65, multi-colour LED feedback, adjustable acoustic feedback. Additional input to actively change the LED colour.

Dimensions: 80 x 80  mm

( ) Flush mounting 12 mm deep
( ) Surface mounting 21 mm deep
( ) Variant for WC
 

or

GEZE LED sensor push button, plastic, IP rating IP 69K

round, diameter: 100 mm

( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm

 

or

GEZE LED sensor push button, glass, IP rating IP 69K

round, diameter: 100 mm

( ) Flush-mounted

( ) Surface-mounted: mounting ring high 20 mm
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Activation (optional position)
GEZE wireless programme with secure rolling code encryption for wireless activation of the drive (approx. 30 m range in the building).

Transmitter:

(  )   Wireless transmitter with 1 key, IP rating IP 54 and wall fixing

(  )   Wireless transmitter with 2 keys, IP rating IP 54 and wall fixing

(  )   Wireless transmitter with 4 keys, IP rating IP 54 and wall fixing

(  )   Transmitting module for optional integration in GEZE elbow switches
Receiver:

(  )   Receiving module with 2 outputs, 24 V, pulse mode or pulse and

       permanent mode for installation in the drive or in a flush-mounted box with IP rating IP 20
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Activation (optional position)

GEZE key switch outside (IP rating IP 54) with or without profile half cylinder and switch function

(  ) Surface-mounted   (  ) Flush-mounted
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Activation (optional position)

GEZE key switch outside (IP rating IP 54) with or without profile half cylinder and hold-open function for the fire service

(  ) Flush-mounted
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	             .........................  pcs.                  ..............................  €             ..............................  €

Activation (optional position)

GEZE key switch outside (IP rating IP 54), prepared for on site profile half cylinder of closing system and 1 push button switch with key symbol for opening from the inside. On contact, the system opens from its locked position once outwards and inwards, and locks again after the leaf has reached the closed position.
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Safeguarding (optional position)

GEZE emergency stop switch with glass pane and lighting for switching off the mains voltage, IP rating IP 20

An emergency command device (emergency stop switch) is not essential in accordance with EN 16005.

(  ) Surface-mounted   (  ) Flush-mounted
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Safeguarding (optional position)

GEZE emergency stop switch with illuminated mushroom button for emergency opening or emergency unlocking, IP rating IP 40

An emergency command device (emergency stop switch) is not essential in accordance with EN 16005.

(  ) Surface-mounted   (  ) Flush-mounted
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Lighting (optional position)

(  ) ..... pcs. LED spotlight (max. 2.6 W per light) integrated in the soffit

or
(  ) ..... pcs. recess for lighting to be installed on site (diameter = ..... mm)
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Locking (optional position)

(  ) Electromagnetic locking, integrated in the drive unit,

     with manual emergency unlocking (standard only in the external door)

and in addition

(  ) Bolt lock for fine-framed door leaves for installation in the bottom door shoe profile,

     prepared for profile cylinder and/or profile half cylinder, lockable on one side

     (profile half cylinder 46 mm long)

or
(  ) Bistable electromechanical rod locking integrated invisibly into the roof or drive cover
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Hot-air curtain system (optional position)

Hot-air curtain system integrated into the ceiling construction of the curved sliding door, with a straight blow-out channel centred on the ceiling (minimum canopy height 400 mm)
Hot-air curtain system design with:

(  ) Electric connection:               Heat output: ............kW/ Amount of air.........m³/h

(  ) Hot water connection            Heat output: ............kW/ Amount of air.........m³/h

Note: The power of the hot-air curtain equipment included in the offer has not been calculated by us; the dimensioning and specification of the hot-air curtains must be carried out by the specialist planner responsible.
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Façade connection (optional position)

(  ) Central façade connection
(..) Off-centre façade connection

(  ) Connections and installation of the curved sliding door off-centre to the façade

and/or

(  ) Larger side parts which turn the arch into an oval system. Details and dimensions on request.
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CAN interface for the connection to the building management

Technical data:

CAN interface galvanically isolated.

CAN extension module for automatic GEZE sliding door, revolving door and swing door drives as interface to connect to the GEZE building management system myGEZE Control.
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Building automation connection

Building automation and control system 
For the integration of escape door control units, swing door drives, sliding doors and automatic window systems into a building management system for the use of typical building automation and control functions.

An automation controller with the following profile must be used:

BACnet device of the type BACnet Building Controller (B-BC) with tested conformity to the BACnet standard ISO 16484-5

myGEZE Control System

...... Piece basic controller as a powerful embedded PC that supports the BACnet protocol. BACnet controller of type B-BC (BACnet Building Controller / protocol audit 14)
for the integration of GEZE field bus devices. The number of fieldbus devices is specified in the specifications.

The system must be able to provide the following components (incl. software licence):

· myGEZE Control basic controller, embedded PC incl. GEZE Library 

· Terminal system for connecting the GEZE CAN bus 

· Terminal system for the connection of GEZE window technology based on 

             the IQ box KNX  

· Terminal system for connecting digital binary input signals to

             Basis of potential-free contacts 

· Terminal system for connecting digital output signals based on
potential-free door closer or changeover contacts 24 V DC     

The number of terminal systems is to be determined by the supplier on the basis of the tendered products at field level.

In top hat rail housing, incl. power supply unit, required auxiliary terminals for internal potential distribution, bus supply and bus termination.

Standard housing dimensions:  W x H x D 300 x 400 x 200 mm 

Supply voltage: 230 V AC 

incl. the following services:
· Project planning and interface configuration of the offered networking system according to GEZE standard.

· Mechanical assembly, electrical connection, commissioning

              ...........  Option                   ..............................  €             ..............................  €

Optional additional services:

Creation of project-specific wiring schematics for product systems

The service includes: 
· Creation of one basic diagram per door type
· Creation of a wiring schematic for the installed door, window and safety technology product systems
· A change index is included; additional changes charged separately
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