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	Pos. no.
	Quantity
	Unit
	Unit price
	
	Total amount
	




Passage height DB:.......... mm (1-leaf 700-3000 mm, 2-leaf 900-3000 mm

	                                        in conjunction with GCprofile Therm 1-leaf 700-1500 mm)
For sliding door elements which are planned near system limits as far as dimensions and leaf weights are concerned, a feasibility study is recommended by the manufacturer before the order is placed.
Version:
(  ) with single roller carriage for leaf weights up to 120 kg
(  ) with double roller carriage for leaf weights up to 120 kg
                   (note: 140 kg only in combination with GCprofile Therm)
Type of installation:
(  ) wall mounting
or
(  ) post-rail construction (façade) 
or
(  ) girder section installation
Door system version:
(  ) single leaf right hand slide to open
(  ) single leaf  left hand slide to open
 (  ) with fixed panels
(  ) with fanlight (only in combination with GCprofile Therm)
Profile system:
(  ) standard ISO profile fine-framed (up to 120 kg leaf weight):
(  ) with 22 mm ISO glass made of (  ) toughened safety glass or (  ) laminated safety glass
or
(  ) mono glass fine-framed (up to 120 kg leaf weight):
(  ) with 10 mm MONO glass made of (  ) toughened safety glass or (  ) laminated safety glass
or
(  ) toughened safety glass clamping profile (up to 120 kg leaf weight):
(  ) with 10 mm toughened safety glass
(  ) with 12 mm toughened safety glass
or 
(  )  profile system GCprofile Therm (up to 140 kg leaf weight)
(  ) with 32 mm toughened safety glass / 3-pane glass
(  ) with 32 mm toughened safety glass / 2-pane glass
Surface of the light alloy parts of the drive and the moving leaves if appropriate:
(  ) anodised EV1 (E6 C-0)    or (  ) RAL ........
Wiring to be carried out on site according to the GEZE cable plan by an electrical contractor
Installation, commissioning and instruction of the operator as well as documentation handover in accordance with EN 16005 by plant fitters or service partner
In accordance with EN 16005:
- the safety analysis must be prepared as a basis for planning and execution
- an inspection must be carried out at least 1 x year and maintenance at least 1 x year
Activation devices:
Outside:
1 push button for opening the door (see 1.4)
1 indicator lamp (red) for visual “OCCUPIED” display, 24 V AC, white
1 emergency opening switch in a lockable box with glass pane (see 1.7)
Inside:
1 push button for opening and closing the door (see 1.4)
1 indicator lamp (red) for visual “OCCUPIED” display, 24 V AC, white

	


	1.0 
	             .........................  pcs.                  ..............................  €             ..............................  €
Operation
GEZE display programme switch in the AS 500 range for setting the mode of operation as well as for commissioning the drive and setting parameters, with function keys, 2x 7-segment display, alphanumerical error display, IP40 rating
Modes of operation: permanently open, automatic, exit only, night-locking, off
(  ) surface mounting      (  ) flush mounting 
or
GEZE keypad programme switch for setting the mode of operation, with function keys, LED dot display, coded error display, IP40 rating, suitable for switch product ranges with 55 x 55 mm switch unit
Modes of operation: off, permanently open, automatic, exit only, night-locking
(  ) surface mounting      (  ) flush mounting 
or
GEZE mechanical programme switch for setting the mode of operation, LED error display, IP40 rating, suitable for switch product ranges with 55 x 55 mm switch insert
Modes of operation : off, permanently open, automatic, exit only, night-locking
(  ) surface mounting      (  ) flush mounting 
(  ) with rotary button      (  ) with key


	1.1 
	             .........................  pcs.                  ..............................  €             ..............................  €
Operation (optional position)
GEZE key switch to “lock” the programme switch to prevent unauthorised changing of the mode of operation, IP40 rating
(  ) surface mounting      (  ) flush mounting
(  ) Euro Profile half cylinder


	1.2 
	             .........................  pcs.                  ..............................  €             ..............................  €
Protection (optional position)
GC 339+ active infrared detector with two light curtains for protecting the opening or closing area in accordance with EN 16005, IP54 rating, 10 possible light curtain configurations
Version:
( ) black
( ) according to RAL
( ) interior ( ) exterior
Accessories:
(  ) outside: weather hood to protect the sensor from the interference of rain
( ) Ceiling installation bracket
( ) Ceiling installation kit for integrating the active infrared detector in the ceiling



	
	

	1.3 
	             .........................  pcs.                  ..............................  €             ..............................  €
Activation (optional position)
GEZE elbow switch, plastic, IP30 rating
Dimensions: 90 x 180 x 23 mm 
(  ) white 
 (  ) stainless steel
( ) optional transmitting module 
(  ) surface mounting
(  ) Rear panel for attaching the elbow switch to glass (in connection with transmitting module)
or
GEZE elbow switch, LS990, IP30 rating
Dimensions: 81 x 223 x 51 mm
(  ) white  
(  ) stainless steel
( ) optional transmitting module 
(  ) surface mounting      (  ) flush mounting
or
GEZE elbow switch, stainless steel, IP65 rating
Dimensions: 72 x 250 x 17 mm 
(  ) surface mounting 
or
GEZE non-contact proximity switch (radar)
Plastic with antimicrobial surface, IP rating IP65, multi-colour LED feedback, adjustable acoustic feedback. Additional input to actively change the LED colour.

Dimensions: 80 x 80  mm

( ) Flush mounting 12 mm deep
( ) Surface mounting 21 mm deep
( ) Variant for WC
or
GEZE LED sensor push button, plastic, IP rating IP 69K
round, diameter: 100 mm
( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm
 
or
GEZE LED sensor push button, glass, IP rating IP 69K
round, diameter: 100 mm
( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm
or
GEZE LED sensor foot switch, glass, IP69K rating

Dimensions: 100 x 100 x 3 mm

(  ) flush mounting
(  ) vertically adjustable installation base for depths of up to 215 mm from the unfinished floor.


	1.4 
	             .........................  pcs.                  ..............................  €             ..............................  €
Protection (optional position)
GEZE protective leaf for protecting against shearing, nipping and trapping positions in accordance with EN 16005 in front of the moving leaf, leaves made of 10 mm toughened safety glass including door fitting, can be turned for cleaning purposes.
When used with the profile systems, the clearances and distances specified in EN 16005 must be observed.

(  ) fastening on the drive or (  ) fastening on the wall
Alternatively:
(  ) sensor-controlled fixed panel protection using 3D light curtain


	1.5 
	             .........................  pcs.                  ..............................  €             ..............................  €
Protection (optional position)
GEZE safety leaf for protecting against shearing and nipping positions in accordance with EN 16005 with post-rail structures (depending on the offset between post surface and façade glazing) behind the moving leaf, leaf made of 10 mm toughened safety glass incl. door fitting
Alternatively:
(  ) sensor-controlled fixed panel protection using 3D light curtain


	1.6 
	             .........................  pcs.                  ..............................  €             ..............................  €
Protection (optional position)
GEZE emergency stop switch with lighting for switching off the mains voltage, IP20 rating
An emergency control device (emergency stop switch) is not essential for compliance with EN 16005.
(  ) surface mounting      (  ) flush mounting


	1.7 
	             .........................  pcs.                  ..............................  €             ..............................  €
Locking (optional position)

(  ) two-stage electromagnetic locking integrated in the drive, with manual emergency unlocking


	1.8 
	             .........................  pcs.                  ..............................  €             ..............................  €
Floor guide (optional position)
Continuous floor guide made of aluminium, anodised  E6 C-0 (EV1), can be installed flush in the floor, guide rail can be removed for cleaning or replaced
Recommended for external doors with opening widths greater than 2000 mm
(  ) with floor guide drainage


	1.9 
	             .........................  pcs.                  ..............................  €             ..............................  €
CAN interface for the connection to the building management

Technical data:
CAN interface galvanically isolated.
CAN extension module for automatic GEZE sliding door, revolving door and swing door drives as interface to connect to the GEZE building management system myGEZE Control.


	1.10 
	             .........................  pcs.                  ..............................  €             ..............................  €

Building automation connection

Building automation and control system 
For the integration of escape door control units, swing door drives, sliding doors and automatic window systems into a building management system for the use of typical building automation and control functions.
An automation controller with the following profile must be used:
BACnet device of the type BACnet Building Controller (B-BC) with tested conformity to the BACnet standard ISO 16484-5

myGEZE Control System
...... Piece basic controller as a powerful embedded PC that supports the BACnet protocol. BACnet controller of type B-BC (BACnet Building Controller / protocol audit 14)
for the integration of GEZE field bus devices. The number of fieldbus devices is specified in the specifications.

The system must be able to provide the following components (incl. software licence):

· myGEZE Control basic controller, embedded PC incl. GEZE Library 
· Terminal system for connecting the GEZE CAN bus 
· Terminal system for the connection of GEZE window technology based on 
             the IQ box KNX  
· Terminal system for connecting digital binary input signals to
             Basis of potential-free contacts 
· Terminal system for connecting digital output signals based on
potential-free door closer or changeover contacts 24 V DC     
The number of terminal systems is to be determined by the supplier on the basis of the tendered products at field level.
In top hat rail housing, incl. power supply unit, required auxiliary terminals for internal potential distribution, bus supply and bus termination.
Standard housing dimensions:  W x H x D 300 x 400 x 200 mm 
Supply voltage: 230 V AC 
incl. the following services:
· Project planning and interface configuration of the offered networking system according to GEZE standard.

· Mechanical assembly, electrical connection, commissioning
              ...........  Option                   ..............................  €             ..............................  €
Optional additional services:

Creation of project-specific wiring schematics for product systems

The service includes: 
· Creation of one basic diagram per door type
· Creation of a wiring schematic for the installed door, window and safety technology product systems
· A change index is included; additional changes charged separately
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