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	Pos no.
	Quantity
	Unit
	Unit price
	
	Total amount
	



	1.0 
	             .........................  Pc.                   ..............................  €             ..............................  €
GEZE AXIRA swing door drive
Single leaf, for on-site pivot doors as a quiet electromechanical drive for interior and exterior doors, in 75 mm overall height, tested and certified according to EN 16005. 
Assembly of the drive system above the door frame in a suspended ceiling or wall structure
Intelligent digital control unit (category 2 according to DIN EN 954-1 and performance level D according to DIN EN ISO 13849-1).
Functions:
Modes of operation: automatic, off (manual movement) adjustable
Special function: automatic locking device for the door leaf in case of wind load, when wind sensor is connected
Obstacle detection and reversal
Diagnostic function and error memory, all settings possible via optional display programme switch
Technical features:
Dimensions: 381 x 276 x 75 mm (L x W x H)
Power supply: 230 V AC, 50/60 Hz
Door leaf width: min./max. 1000/2400 mm,
Leaf height: min/max. 2000/4000 mm
Door weight: max. 450 kg 
Door opening angle: 90° recommended (an opening angle ≥ 90° leads to reduced clear passage width)
Opening and closing time adjustable
electrical latching action adjustable
hold-open time adjustable from 0 to 60 seconds
Possible connections:
Separate inputs for internal and external sensors
Emergency stop switch, programme switch, on-site motor lock, on-site electric strike, power supply for external devices: 24 V DC, 1200 mA continuous, 1800 mA short-term
Wiring to be carried out on site by an electrical contractor according to the GEZE cable plan, commissioning to be carried out by plant fitters or service partner.
According to EN 16005, the following must apply:
- Safety analysis must be carried out as a basis for planning and execution
- Maintenance and accident prevention (UVV) inspection must be carried out at least 1 x year
- The secondary closing edge of an automatic swing leaf door must be safeguarded
If there is no protection, the safety analysis must refer to the residual risk.
Safeguarding of the secondary closing edge is to be carried out on site and is not part of the scope supplied by GEZE GmbH.
Note on locking:
Electric strike, for releasing the door, 24 V DC, as a counterpart to the latch lock, as well as lock switch contact to switch off the drive when the door is locked (1 piece per drive) must be provided.


	1.1 
	             .........................  pcs.                  ..............................  €             ..............................  €
Protection (optional position)

GEZE GC 342 laser scanner, tested in accordance with EN 16005, mounted on the door leaf, to protect the swivelling range of interior and exterior doors in the opening and closing direction. Robust enough to handle all floor conditions (e.g. entrance mat, metal rail, dark and absorbing flooring, shiny and wet tiles, grating). With integrated wall blanking and dynamic main closing edge protection.
 
Door leaf width: ....... mm
( ) GC 342 laser scanner kit (contains two sensors to protect both sides of the leaf)
IP rating IP54, with optimised secondary closing edge protection. If fingers are very likely to be trapped on the secondary closing edge, a combination with GC 342+ can be considered
( ) GC 342 for hinge side and GC 342+ for the opposite hinge side
Combination of GC 342, IP rating IP54 for the hinge side and GC 342+, IP rating IP44 for the opposite hinge side. Each as an individual module (left and right variants)
Version:
( ) stainless steel colour
( ) black
( ) white
 
( ) Fire protection kit - master-slave replacement cable which enables cables to be guided through 5 mm instead of 10 mm bore-holes. The drilling permit must be requested from the door manufacturer.
Only available for GC 342:
Protective cover to protect the laser scanner against interferences
( ) stainless steel colour
( ) black
( ) according to RAL
 
( ) Retrofit interface - retrofit circuit board for connection to door cables fitted on site


	1.2 
	             .........................  pcs.                  ..............................  €             ..............................  €
Safeguarding (optional position)
GEZE emergency stop switch with glass pane and lighting for switching off the mains voltage, IP rating IP 20
(  ) Surface-mounted   (  ) Flush-mounted
An emergency command device (emergency stop switch) is not essential for compliance with EN 16005.


	1.3 
	             .........................  pcs.                  ..............................  €             ..............................  €

Activation (optional position)

GC 308 radar movement detector with direction detection and cross-traffic fade-out for activation, IP 54 rating, multi-colour LED feedback

Dimensions (WxHxD): 120 x 50 x 50 mm

Version:

(  ) black 

(  ) white 

(  ) stainless steel colour 

(  ) acc. to RAL

(  ) outside   (  ) inside

Accessories:

(  ) Ceiling installation kit

(  ) Ceiling bracket

(  ) exterior: weather hood


	1.4 
	             .........................  pcs.                  ..............................  €             ..............................  €

Activation (optional position)

GC 302 radar movement detector with direction detection and cross-traffic fade-out for activation, IP rating IP 54

Dimensions (WxHxD): 176 x 62 x 52 mm

Version:

(  ) black 

(  ) acc. to RAL

(  ) outside   (  ) inside

Accessories:

(  ) Ceiling installation kit

(  ) exterior: weather hood


	1.5 
	             .........................  pcs.                  ..............................  €             ..............................  €
Activation (optional position)

GEZE elbow switch, plastic, IP rating IP 30

Dimensions: 90 x 180 x 23 mm 

( ) white  ( ) stainless steel

( ) optional transmitting module 

( ) Surface-mounted  ( ) Rear panel for attaching the elbow switch to glass (in connection with the transmitting module)

or
GEZE elbow switch, LS990, IP rating IP 30

Dimensions: 81 x 223 x 51 mm

( ) white  ( ) stainless steel

( ) optional transmitting module 

( ) Surface-mounted ( ) Flush-mounted

or
GEZE elbow switch, stainless steel, IP rating IP 65

Dimensions: 72 x 250 x 17 mm 

( ) Surface-mounted

 

or
GEZE non-contact proximity switch (radar)

Plastic with antimicrobial surface, IP rating IP65, multi-colour LED feedback, adjustable acoustic feedback. Additional input to actively change the LED colour.

Dimensions: 80 x 80  mm

( ) Flush mounting 12 mm deep
( ) Surface mounting 21 mm deep
( ) Variant for WC
 

or
GEZE LED sensor push button, plastic, IP rating IP 69K
round, diameter: 100 mm
( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm
 
or
GEZE LED sensor push button, glass, IP rating IP 69K
round, diameter: 100 mm
( ) Flush-mounted

( ) Surface-mounted: mounting ring flat 4 mm

( ) Surface-mounted: mounting ring high 20 mm
or
GEZE LED sensor foot switch, glass, IP rating IP69K
Dimensions: 100 x 100 x 3 mm

( ) flush-mounting

( ) vertically adjustable installation base for depths of up to 215 mm from the unfinished floor


	1.6 
	             .........................  pcs.                  ..............................  €             ..............................  €
Activation (optional position)
GEZE wireless programme with secure rolling code encryption for wireless activation of the drive (approx. 30 m range in the building).
Transmitter:
(  ) Hand-held transmitter with 1 key, IP rating IP 54 and wall fixing
(  ) Hand-held transmitter with 2 keys, IP rating IP 54 and wall fixing
(  ) Hand-held transmitter with 4 keys, IP rating IP 54 and wall fixing
(  ) Transmitting module for optional integration in the GEZE elbow switch (not for elbow switch variant stainless steel IP 65)
Receiver:
(  ) Receiving module with 2 outputs, 24 V, pulse mode or pulse and permanent mode for installation in the drive or in a flush-mounted box with IP rating IP 20


	1.7 
	             .........................  pcs.                  ..............................  €             ..............................  €
Activation (optional position)

GEZE GCER 300, 1-door SET
Access control solution with RFID reader and PIN keypad in stand-alone operation for controlling one door (can be extended to 2 doors). RFID frequency 13.56 MHz. Authorisation is granted through master ID cards in combination with PIN keyboard directly at the reader. Up to 200 persons/ID cards can be authorised. If individual ID cards are lost or become faulty, they can simply be deleted from the system (selective deletion). Two authorisation types for short-time release or continuous release (office function). Configurable door release time. Variable PIN length. Communication between reader and control unit takes place by encrypted data transfer. Functions such as interlocking door system or dementia adjustable. Release buttons can be connected.
Set comprising:
1 pc. GEZE GCER 300 I/O Box (ID no. 185707)
1 pc. GEZE GCVR 300 T, RFID reader flush-mounted (ID no. 185708)
2 pc. GEZE GCER 300 system card master (ID no. 185713)
10 pc. GEZE RFID ID card (ID no. 185711)
Optional
GEZE GCVR Touch 300 T, RFID reader flush-mounted (ID no. 187108)
GEZE RFID key fob (ID no. 185712)
GEZE GCER AP surface-mounted frame (Id. no. 130024)

or

GEZE GCER 300 Light, 1-door SET
Access control solution with RFID reader and PIN keyboard in stand-alone operation with a relay output for controlling one door located in the secured inner area. RFID frequency 13.56 MHz. Authorisation is granted through master ID cards in combination with PIN keyboard directly at the reader. Up to 200 persons/ID cards can be authorised for short-time release. If individual ID cards are lost or become faulty, they can simply be deleted from the system (selective deletion). Configurable door release time. Variable PIN length. Communication takes place via encrypted data transfer.
Set comprising:
1 pc. GEZE GCER 300 Light, RFID reader flush-mounted (ID no. 185710)
1 pc. GEZE GCER 300 system card master (ID no. 185713)
10 pc. GEZE RFID ID card (ID no. 185711)
Optional
GEZE RFID key fob (ID no. 185712)
GEZE GCER AP surface-mounted frame (ID no. 130024)

Accessories for GCER 300 / GCER 300 Light
Plug-in power supply NT 1.0 A – 24 V DC (optional)
Primary:  230 V AC, 50 Hz
Secondary: 24 V DC (+/- 5 %) / 1 A
(ID no. 130025)

Power supply NT 1.1 A – 24 V DC flush-mounted (optional)
For installation in deep standard flush-mounted boxes
Primary:  230 V AC, 50 Hz
Secondary: 24 V DC / 1.1 A
(ID no. 151426)
Power supply NT 1.5 A – 24 V DC HA (optional)
For installation on top hat rails 
Primary: 230 V AC, 50 Hz
Secondary: 21.6 – 26.4 V DC / 1.5 A
(ID no. 151425)



	1.8 
	             .........................  pcs.                  ..............................  €             ..............................  €

Opening restrictor (optional position, an opening restrictor is necessary)

GEZE door stop, to protect the door and its direct environment.



	1.9 
	             .........................  pcs.                  ..............................  €             ..............................  €

Opening restrictor (optional position, an opening restrictor is necessary)

GEZE integrated opening restrictor, can also be retrofitted to the guide rail on site.

Area of application: internal doors



	1.10 
	             .........................  pcs.                  ..............................  €             ..............................  €
Operation (optional position)
GEZE display programme switch in the AS 500 range for setting the mode of operation as well as for commissioning and setting the parameters of the drive, with control keys, 2x 7-segment display, alphanumerical fault display, IP rating IP 40
Operating modes: off, permanently open, automatic, shop closing, night-locking
(  ) Surface-mounted (  ) Flush-mounted
or
GEZE mechanical programme switch for setting the operating mode, with rotary button, LED fault display, IP rating IP 40, suitable for switch programmes with 55 x 55 mm switch insert
Operating modes: off, permanently open, automatic, shop closing, night-locking
(  ) Surface-mounted   (  ) Flush-mounted
or
GEZE mechanical programme switch for setting the operating mode, with key, LED fault display, IP rating IP 40, suitable for switch programmes with 55 x 55 mm switch insert
Operating modes: off, permanently open, automatic, shop closing, night-locking
(  ) Surface-mounted   (  ) Flush-mounted


	1.11 
	             .........................  pcs.                  ..............................  €             ..............................  €
Operation (optional position)
GEZE key switch to “lock” the programme switch to prevent unauthorised changing of the operating mode, IP rating IP 40
(  ) Surface-mounted   (  ) Flush-mounted


	1.12 
	             .........................  pcs.                  ..............................  €             ..............................  €
CAN interface for the connection to the building management

Technical data:
CAN interface galvanically isolated.
CAN extension module for automatic GEZE sliding door, revolving door and swing door drives as interface to connect to the GEZE building management system myGEZE Control.


	1.13 
	             .........................  pcs.                  ..............................  €             ..............................  €

Building automation connection

Building automation and control system 
For the integration of escape door control units, swing door drives, sliding doors and automatic window systems into a building management system for the use of typical building automation and control functions.
An automation controller with the following profile must be used:
BACnet device of the type BACnet Building Controller (B-BC) with tested conformity to the BACnet standard ISO 16484-5

myGEZE Control System
...... Piece basic controller as a powerful embedded PC that supports the BACnet protocol. BACnet controller of type B-BC (BACnet Building Controller / protocol audit 14)
for the integration of GEZE field bus devices. The number of fieldbus devices is specified in the specifications.

The system must be able to provide the following components (incl. software licence):

· myGEZE Control basic controller, embedded PC incl. GEZE Library 
· Terminal system for connecting the GEZE CAN bus 
· Terminal system for the connection of GEZE window technology based on 
             the IQ box KNX  
· Terminal system for connecting digital binary input signals to
             Basis of potential-free contacts 
· Terminal system for connecting digital output signals based on
potential-free door closer or changeover contacts 24 V DC     
The number of terminal systems is to be determined by the supplier on the basis of the tendered products at field level.
In top hat rail housing, incl. power supply unit, required auxiliary terminals for internal potential distribution, bus supply and bus termination.
Standard housing dimensions:  W x H x D 300 x 400 x 200 mm 
Supply voltage: 230 V AC 
incl. the following services:
· Project planning and interface configuration of the offered networking system according to GEZE standard.
· Mechanical assembly, electrical connection, commissioning
              ...........  Option                   ..............................  €             ..............................  €
Optional additional services:

Creation of project-specific wiring schematics for product systems
The service includes: 
· Creation of one basic diagram per door type
· Creation of a wiring schematic for the installed door, window and safety technology product systems
· A change index is included; additional changes charged separately
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