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	Object:
	

	Support:
	

	Spec. no.:
	
	Location:
	


_________________________________________________________________________________

Pos. no.		Quantity		Unit   	Unit price		Total amount
_________________________________________________________________________________


   
	1.0 
	                ..........               Pcs                     €..................                     €..................

Surface housing

e.g. for installation of cap rail power supplies or other electronic cap rail components with the max. dimensions of approx 119 x 93 x 55 mm.
Aesthetic design.

Technical data:
Plastic casing white, cascading
Cable feed surface or floating

Design:
Dimensions W x H x D [mm]: approx. 193 x 130 x 82
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