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	1.0 
	Building management system for visualisation and alarm processing 
Server and client-based building management system for monitoring, controlling, visualisation and processing alarms for product systems connected via the BACnet data protocol.  
The myGEZE Visu server serves as the central hub, storing system
master data as well as logs, events and statuses in the database. It uses a driver to link to the connected systems.
The systems are configured and managed using a program 
that communicates with the server to be configured via an IP connection. The 
configuration can be completed during ongoing operation. 
Users can use the server on one or more client systems. The generated system graphics are visualised on the client systems. Intuitively designed interfaces are used for operation and monitoring. A menu-guided workflow is available for handling alarms, faults and events.
· Server and client-based application for communication with GEZE product systems and BACnetIP-based visualisation and control devices.
· Separately licensable and expandable software options.
· With optional hardware for installation in closed control cabinets
Communication with lower-level product systems is handled via the standardised data transfer protocol in accordance with BACnet standard 16484-5 in BACnet Protocol Revision with at least version 12.


	1.1 
	myGEZE Visu basic software package 
Software package for status visualisation and operation of connected product systems, consisting of:
· myGEZE Visu Server incl. all system components
· Drivers for GEZE product systems
· Pre-definition for system, product group, stations, data point types
· 1x myGEZE Visu client system
· Representation of views, system visualisation
· User system with authorisation via operator, groups, roles
· Pre-defined message handling, workflow for troubleshooting faults
· Email notification to send alarms, messages, events
· License to connect a max. of 5 GEZE product systems
· Option to expand to a max. of 200 connected GEZE product systems
· Option to expand with additional myGEZE Visu client operating stations
· Option to expand with user system client-capability
· Option to expand by connecting multi-monitor systems
Delivered as an installation package for installation on provided computer systems.
The minimum system requirements must be complied with.
Minimum service requirement: myGEZE Visu basic setup for status visualisation and operation of connected product systems
Product: myGEZE Visu basic software package or equivalent
 
.........................  pcs.                   ..............................  €             ..............................  €


	1.2 
	myGEZE Visu licence option Number of product systems
License expansion for basic software or hardware package to connect additional GEZE product systems 

· Expansion package for one of the basic packages to connect additional GEZE product systems
· myGEZE Visu Client operating stations
· Available in the versions 5, 10, 25, 50, 200 product systems
Product: myGEZE Visu licence option Number of product systems
.........................  Option                   ..............................  €             ..............................  €


	1.3 
	myGEZE Visu Client licence option
License expansion for the basic software or hardware packages to use an additional myGEZE Visu Client operating station
Product: myGEZE Visu licence option Client
.........................  Option                   ..............................  €             ..............................  €


	1.4 
	myGEZE Visu licence option 5 Client
License expansion for the basic software or hardware packages to use 5 additional myGEZE Visu Client operating stations as a bundle
Product: myGEZE Visu licence option 5 Client
.........................  Option                   ..............................  €             ..............................  €


	1.5 
	myGEZE Visu licence option Client capability

License expansion for basic software or hardware package to use client management in the user system
 
· 32 client groups
· Domain connection to log in with domain user (Windows login)
· Client function organises the visibility of
· Views (drawings, individual layers, symbols)
· System visualisations
· Data points
· Event information
· System information and system menus
Product: myGEZE Visu licence option Client capability
........................  Option                   ..............................  €             ..............................  €


	1.6 
	myGEZE Visu licence option multi-monitor

License expansion for basic software or hardware package to use a multi-monitor system
 
· Option to allocate different parts of the system to different monitors
· Up to 4 monitors possible
· It may not be possible to allocate all parts of the system with free variability in some systems
Product: myGEZE Visu multi-monitor licence option
........................  Option                   ..............................  €             ..............................  €


	1.7 
	myGEZE Visu video integration licence option

License expansion for basic software or hardware package to integrate digital video systems
 
· Option to integrate digital video systems 
· Depending on the system requirements, the following video drivers are possible: RTSP, DVMS, ONVIF, HTML, VNC, Avigilon, Cayuga, Bosch, Hikvision
Product: myGEZE Visu video integration licence option
........................  Option                   ..............................  €             ..............................  €


	1.8 
	Service configuring the building management system 
Base configuration of myGEZE Visu for status visualisation and operation of connected product systems 
Base configuration consisting of:
· Database configuration of the connected BACnet controllers type myGEZE Control

· Setting up project-specific network settings

· Create and name an admin user

· Create and name another user

· Creating and labelling a role

· Setting up a client

· Creating an alarm stack
Product: myGEZE Visu base configuration
........................  pcs.                   ..............................  €             ..............................  €


	1.9.1

	Visualisation page set-up
 
Set-up includes the following activities:
· Creation of configured number of levels or
· Creation of configured number of rooms or
· Creation of configured number of departments
· Integration of configured number of basic layouts after provision on-site
 Product: Setup of configured num. Visualisation page
........................  pcs.                   ..............................  €             ..............................  €


	1.9.2
	Setting up of device panel for operation and status visualisation // Template
 
· Configuration of the device template
· Designate and link properties
· Locate in the building structure

 Product: Setup of configured number of device panels
........................  pcs.                   ..............................  €             ..............................  €


	1.9.3
	Base configuration of scene
· Creation of configured number of scene according to technical specification
Product: Setup of configured number of scenes
........................  pcs.                   ..............................  €             ..............................  €


	1.9.4
	Setup of a time-controlled function for connected product systems
 
· Create timer function according to the configured number
 Product: timer
........................  pcs.                   ..............................  €             ..............................  €


	1.9.5
	Set up a calendar-driven function for connected product systems

· Create calendar function according to configured number
Product: Calendar function
........................  pcs.                   ..............................  €             ..............................  €


	1.9.6
	Basic setup of alarms / Setting up an alarm

Base configuration consisting of:

· Set up alarm type according to configured number

· Create alarm and define output

Product: Basic setup / Setting up an alarm according to the configured number
........................  pcs.                   ..............................  €             ..............................  €



	1.9.7
	Base configuration of email notification
Base configuration consisting of:
· Basic setup of email server according to the configured number
· Creating recipient contact according to the configured number  
 Product: Base configuration of email notification according to the configured number
........................  pcs.                   ..............................  €             ..............................  €



	1.9.8
	Creating an additional user
 
· Creating an additional user and assigning a role and optional client according to the configured number

 Product: Creating a user according to the configured number
........................  Option                   ..............................  €             ..............................  €



	1.9.9
	Creating a user role
 
· Creating an additional user role according to the configured number
· Assigning user rights according to the configured number 

 Product: Creating a user role according to the configured number 
........................  Option                   ..............................  €             ..............................  €



	1.9.10
	Creating a client (optional – only if licensing package ordered)
 
· Creating additional clients according to the configured number 
· Assigning levels/rooms/department to client according to the configured number 

 Product: Creating a client according to the configured number 
........................  Option                   ..............................  €             ..............................  €


	1.9.11
	Workflow configuration

· Adjustment of the system-related alarm workflow according to user specifications

Product: Create workflow according to configured number
........................  Option                   ..............................  €             ..............................  €



	1.9.12
	Installation of additional operating stations

· Install additional operating stations / clients according to the configured number

· Connect additional operating stations to the server system according to the configured number

Product: Create client according to configured number

........................  Option                   ..............................  €             ..............................  €



	1.9.13
	Screen layout
· Delivery in the standard layout L1; alternatives: L2, L4, ...
· Deviating layout desired: yes/no
Product: Creating a screen layout
........................  Option                   ..............................  €             ..............................  €



	1.9.14
	Custom programming
· Completion of additional work on an hourly basis after approval of the technical specification.
· This work is billed by the hour, based on actual hours worked.
Product: Custom programming, based on time sheet
........................  Option                   ..............................  €/hr.      ..............................  €



	1.9.15
	Travel and setup flat rates
· Travel and setup flat rates for travel to the building site for commissioning, construction meetings and coordination meetings
 ........................  Option                   ..............................  €/hr.      ..............................  €
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